9.14.2026
Question & Answer
Questions and clarifications about the project
The question submission deadline has passed. No more questions can be submitted.
1. Pre-Bid Aug 25 2026 at 12:55 PM
· 
Anonymous Aug 25 2026 at 12:55 PM
User information is private
Can the Pre-Bid Meeting be made mandatory for all prospective bidders? Important project information, clarifications, and discussions regarding the scope of work are often addressed during the Pre-Bid Meeting. Requiring all bidders to attend would help ensure that each bidder receives the same information and is bidding on an equal and consistent basis.
· 
Aug 25 2026 at 2:07 PM
Escambia County
No, the county does not wish this to be a mandatory pre-solicitation. If we make the pre-solicitation mandatory, then we are drastically limiting the bidder pool. The county feels there is enough information in the plans, specs, etc. that bidders can determine what questions they need to ask before the question and answer due date without having a mandatory pre-solicitation. 
2. Budget  Aug 26 2026 at 7:38 AM
· 
Anonymous Aug 26 2026 at 7:38 AM
User information is private
What is the County's budget for this project? 
· 
Aug 26 2026 at 12:05 PM
Escambia County
This is a formal solicitation so the county expects the budget to be over $50,000.
3. Signage  Aug 26 2026 at 9:04 AM
· 
Anonymous Aug 26 2026 at 9:04 AM
User information is private
There is a reference to a digital sign on sheet T101, where is the detail for the digital sign? 
· 
Sep 1 2026 at 10:41 AM
Escambia County
Please disregard this note. There is no corresponding reference on the plan.
4. Exterior/Interior Building Sign  Aug 26 2026 at 9:04 AM
· 
Anonymous Aug 26 2026 at 9:04 AM
User information is private
Please provide details to the building signage 
· 
Sep 1 2026 at 10:41 AM
Escambia County
Sign specs are called out on sheet A201.
5. Budget & Design Aug 26 2026 at 9:32 AM
· 
Joshua Owens Aug 26 2026 at 9:32 AM
GSI Construction Corporation, Inc
Your information is only visible to you
With Fire Station 20 being cancelled after bid due to costs exceeding the budget, will this Fire Station need redesign in order to fall within budget?
· 
Sep 1 2026 at 10:41 AM
Escambia County
There will be no redesign.
6. Sectional Overhead Doors Aug 26 2026 at 4:28 PM
· 
Anonymous Aug 26 2026 at 4:28 PM
User information is private
#1) Do the Sectional Overhead Door(s) Type J require “Energy Code Compliance”: Air Infiltration Resistance for IECC, ASHREA, Florida Energy Code, per NFRC 400, ASTM E283, or DASMA 105? 
· 
Sep 1 2026 at 10:41 AM
Escambia County
It is our understanding that garage doors can be accepted under the following standards: Garage doors 0.40 cfm/ft² ANSI/DASMA 105, NFRC 400, or ASTM E283 A garage door can demonstrate its required air leakage using ANSI/DASMA 105 or ASTM E283 rather than NFRC 400. The specification calls for compliance with ASTM E283, doors must comply with this standard.
7. Sectional Overhead Doors Aug 26 2026 at 4:29 PM
· 
Anonymous Aug 26 2026 at 4:29 PM
User information is private
Do the Sectional Overhead Door(s) Type Jrequire “Water Infiltration Resistance” per ASTM E331 & ASTM E547?
· 
Sep 1 2026 at 10:41 AM
Escambia County
It is our understanding that garage doors can be accepted under the following standards: Garage doors 0.40 cfm/ft² ANSI/DASMA 105, NFRC 400, or ASTM E283 A garage door can demonstrate its required air leakage using ANSI/DASMA 105 or ASTM E283 rather than NFRC 400. The specification calls for compliance with ASTM E283, doors must comply with this standard.
8. Sectional Overhead Doors Aug 26 2026 at 4:39 PM
· 
Anonymous Aug 26 2026 at 4:39 PM
User information is private
Verify the PSF's for Door Type J as +41.7/-45.85?
· 
Sep 1 2026 at 10:41 AM
Escambia County
See diagram on S001, one of the doors falls into a corner zone.
9. “Sectional Overhead Door” Type J:  Aug 27 2026 at 7:33 AM
· 
Joshua Owens Aug 27 2026 at 7:33 AM
GSI Construction Corporation, Inc
Your information is only visible to you
#1) Do the Sectional Overhead Doors Type J require “Energy Code Compliance”: Air Infiltration Resistance for IECC, ASHREA, HVAC Standards; with NFRC certification? Florida State Specific Energy Code, per NFRC 400, ASTM E283, or DASMA 105? #2) Do the Sectional Overhead Doors Type J require “Water Infiltration Resistance” per ASTM E331 & ASTM E547? #3) Verify the PSF’s (pressures) of Door Type J as +41.70/-45.85? 
· 
Sep 1 2026 at 10:41 AM
Escambia County
It is our understanding that garage doors can be accepted under the following standards: Garage doors 0.40 cfm/ft² ANSI/DASMA 105, NFRC 400, or ASTM E283 A garage door can demonstrate its required air leakage using ANSI/DASMA 105 or ASTM E283 rather than NFRC 400. The specification calls for compliance with ASTM E283, doors must comply with this standard. See diagram on S001, one of the doors falls into a corner zone.
10. Allowances Aug 27 2026 at 8:39 AM
· 
Anonymous Aug 27 2026 at 8:39 AM
User information is private
Please confirm whether any allowances will be issued by addendum. If so, should all allowances be included in our total bid amount on bid day, or will the County add them to the awarded bidder’s final contract amount?
· 
Sep 1 2026 at 10:41 AM
Escambia County
The following Allowances are included in the bid. 1. Brick - $800 per thousand 2. Security Engineering - $225,000 3. 10% Owner’s Contingency
11. Bid Time Aug 28 2026 at 12:44 AM
· 
Anonymous Aug 28 2026 at 12:44 AM
User information is private
Can the bid time be moved to the more customary 2:00 pm?
· 
Aug 28 2026 at 9:15 AM
Escambia County
Not at this time. We conduct all bid openings during normal business hours. In this case, the scheduled time is based on personnel availability.
12. Questions & Answers Aug 28 2026 at 12:46 AM
· 
Anonymous Aug 28 2026 at 12:46 AM
User information is private
Can a PDF file of all questions and answers be published for download at the end of the question and answer period?
· 
Aug 28 2026 at 9:17 AM
Escambia County
All questions and answers are downloaded as printable report to the addendum section of the solicitation after Q&A period has ended.
13. Flooring Aug 28 2026 at 2:19 PM
· 
Anonymous Aug 28 2026 at 2:19 PM
User information is private
There is porcelain tile listed on the Flooring Legend on page A106. Is it supposed to be used somewhere, and they didn't put that on the plans?
· 
Sep 11 2026 at 4:11 PM
Escambia County
Porcelain tile can be omitted from the plans, since the toilet rooms were changed to epoxy.
14. Epoxy Flooring Aug 28 2026 at 2:20 PM
· 
Anonymous Aug 28 2026 at 2:20 PM
User information is private
The epoxy flooring in the Apparatus Bay is not supported and warranted, by Neogard, in this area as it is not strong enough to uphold the traffic in that space. Is there another system recommended for that space? 
· Question is acknowledged
15. PEMB Purchase Aug 31 2026 at 1:36 PM
· 
Joshua Owens Aug 31 2026 at 1:36 PM
GSI Construction Corporation, Inc
Your information is only visible to you
I believe it was stated in the prebid meeting that the county would direct purchase the PEMB. 1) Does this include the PEMB insulation? 2) Does this mean the County will select a PEMB vender for purchase, or with the GC need to carry their PEMB vender cost, and then the County will enter into PO with the GC's vender after award? 3) If the County is purchasing the PEMB directly to help avoid the project going over budget, the County may want to direct purchase the same way they are purchasing the HVAC equipment, so that PEMB material costs are NOT included in the GC's bid cost.
· 
Sep 11 2026 at 4:12 PM
Escambia County
1) PEMB insulation will be included in Owner purchase. 2) The County will be putting the metal building out for bid, the Contractor should not include the metal building in the price. 3) Correct, not included.
16. Request for Approval of PEMB Manufacturer Aug 31 2026 at 2:12 PM
· 
Anonymous Aug 31 2026 at 2:12 PM
User information is private
We would like to request that ProSpan Steel Buildings be considered an approved Pre-Engineered Metal Building manufacturer for this project.
· 
Sep 11 2026 at 4:12 PM
Escambia County
Approved, provided they meet all requirements of the original project specifications.
17. Builder's Risk Sep 4 2026 at 2:03 PM
· 
Joshua Owens Sep 4 2026 at 2:03 PM
GSI Construction Corporation, Inc
Your information is only visible to you
Is Builder's Risk by the Owner?
· 
Sep 10 2026 at 7:52 AM
Escambia County
Yes, Builder's Risk will be provided by the Owner for this project. 
18. Bid Date Sep 8 2026 at 9:08 AM
· 
Anonymous Sep 8 2026 at 9:08 AM
User information is private
Would it be possible to move the bid date from Friday the 25th to Monday the 28th?
· 
Sep 8 2026 at 9:19 AM
Escambia County
There are no plans to change the bid opening at this time.
19. Glass/Glazing Sep 8 2026 at 8:45 AM
· 
Anonymous Sep 8 2026 at 8:45 AM
User information is private
Window HH is on the A-301 window schedule (14'-4" sloped clerestory) but is not tagged on any plan or elevation we can find. Please advise where this window is located. 
· 
Sep 11 2026 at 4:12 PM
Escambia County
The window lettering on Sheet A301 is incorrect. These three windows should be labeled FF, GG, and HH.
20. Glass/Glazing Sep 8 2026 at 8:45 AM
· 
Anonymous Sep 8 2026 at 8:45 AM
User information is private
A-301 type DD is drawn 12'-0" x 3'-10", 4 lites. The A-402 wellness elevation shows an untagged 18'-0" x 5'-0" 5-lite band at the same Corridor 136 wall. Which one governs?
· 
Sep 11 2026 at 4:12 PM
Escambia County
Provide Window Type DD as indicated on Sheet A301. The referenced interior elevation, 135A/A402, is located within the Wellness Room and depicts the interior mirror wall.
21. Glass/Glazing Sep 8 2026 at 8:46 AM
· 
Anonymous Sep 8 2026 at 8:46 AM
User information is private
Spec 088000 article 2.10.A: the large missile Low-E insulating glass lists overall unit thickness 1 9/16 inch (25 mm). Those do not match, and the interlayer makeup for the large missile rating is not listed. What IGU makeup and thickness is required?
· 
Sep 11 2026 at 4:12 PM
Escambia County
Total thickness is 1-5/16”. Exterior lite is 1/4” low-e, 1/2” air space, 9/16” impact layer including .090” PVB.
22. Glass/Glazing Sep 8 2026 at 8:46 AM
· 
Anonymous Sep 8 2026 at 8:46 AM
User information is private
The glazed partition at the Kitchen 127 west wall to Corridor 120, with door 120A at its north end, has no tag and no A-301 schedule row. Is it in Division 08 scope, and what type applies?
· 
Sep 11 2026 at 4:12 PM
Escambia County
This is not a glazed partition; it is a double metal stud wall for sound protection.
23. No subject Sep 8 2026 at 8:47 AM
· 
Anonymous Sep 8 2026 at 8:47 AM
User information is private
The kitchen pass window to Dining 126 (elevation 127C/A-402) has no mark or schedule row. Please indicate what type.
· 
Sep 11 2026 at 4:12 PM
Escambia County
This window is noted at Type EE on sheet A101.
24. Glass/Glazing Sep 8 2026 at 8:47 AM
· 
Anonymous Sep 8 2026 at 8:47 AM
User information is private
Door 127B is tagged on rear elevation 1/A-202 with full-height sidelites but has no A-301 row. What size and hardware set apply? Window EB beside it has no schedule row either.
· 
Sep 11 2026 at 4:12 PM
Escambia County
Per sheet A101, the door tag on sheet A201 should read 127A.
25. Glass/Glazing Sep 8 2026 at 8:48 AM
· 
Anonymous Sep 8 2026 at 8:48 AM
User information is private
Door 123A: the schedule remark reads Clopay steel insulated door, the type H caption reads Cornell. Which governs?
· 
Sep 11 2026 at 4:12 PM
Escambia County
Cornell is correct. The Clopay door was unable to meet the wind load.
26. Glass/Glazing Sep 8 2026 at 8:48 AM
· 
Anonymous Sep 8 2026 at 8:48 AM
User information is private
Small untagged opening in the south exterior wall at Toilet 103 on 5/A-107. Louver or window? Please provide additional details.
· 
Sep 11 2026 at 4:12 PM
Escambia County
There is no window or louver on this wall.

